This is Circuitmaker/Traxmaker 2000

Install Circuitmaker/Traxmaker on your hard drive as follows (circle each step number as you do the installation):

1. Click on SetupCM2000.exe.

2. Install the PROFESSIONAL version by using the following:

The access code for this program is YX86 Z8X2 Q6AB WFLR

The serial is 800054.

3. The program will install into "Program Files" "Circuitmaker 2000" (abbreviated here CMTM2K).

4. Copy "Manuals PDF" into the CMTM2K folder in Program Files.

5. In the CMTM2K folder installed onto your hard drive, there is a subfolder called "Models". Rename this subfolder "ModelsOld".

6. Open the "Updates" folder.

7. Copy the "Models" file in "Updates" to the CMTM2K folder in Program Files.

8. Copy the cm2000servicepack 1.exe file to the CMCM2K folder in Program Files.

9. Run the service pack exe file. Allow it to make the backup directory.

10. Open the "File Updates" folder.

11. Copy all the files in the "File Updates" folder into the CMTM2K folder in Program Files (overwrite).

12. Close the Circuitmaker 2000 folder that you got when you unzipped the Schematic & PCB.zip but save it on your hard drive where you can find it if you need it.

13. Go into the Start menu, All Programs, Circuitmaker, and drag an icon to both Circuitmaker and Traxmaker onto your desktop screen.